Audio parameter:

Audio parameters can be divided into two parts, one part is in this file

/device/sprd/sharkle/sp9820e\_2c10/modem\_bins/ltenvitem.bin ---Parameters about Call/talking.

Other part is about MP3/MP4 etc. and is stored at below path:

/device/sprd/sharkle/sp9820e\_2c10/rootdir/system/etc/audio\_params/

/device/sprd/sharkle/sp9820e\_2c10/rootdir/system/etc/audio\_policy\_config/

RF:

All RF parameters are include in this file:

/device/sprd/sharkle/sp9820e\_2c10/modem\_bins/ltenvitem.bin

Camera:

For all sensors, their parameters and drivers are at below path：

vendor/sprd/modules/libcamera/sensor/sensor\_drv/classic/Superpix/

/vendor/sprd/modules/libcamera/sensor/sensor\_drv/classic/Galaxycore/