

AP+ MODEM (Logs)


Insert SD card (above 4G)

Input secret code \*#\*#0574#\*#\* for enter Log Manager setting UI

Select Log Switch , and select option as below snapshot.

**AP Log Settings:**



Then test, if issue happened , copy logs out from SD card and share to us.

**Modem logs tool**---------please find it at below address:

/data/F271i/Tool/Logel\_for\_TD\_W18.52.2.rar

**SFTP:**

              Server IP : 49.40.21.34

  Port   : 5522

              Username: Mega\_tech

              Password: AA$$jj11