**For all partition info you can refer below list:**

<!-- size unit is MBytes   -->

  <Partition id="**prodnv**" size="**5**" />

  <Partition id="**miscdata**" size="**1**" />

  <Partition id="**recovery**" size="**19**" />

  <Partition id="**misc**" size="**1**" />

  <Partition id="**trustos**" size="**6**" />

  <Partition id="**trustos\_bak**" size="**6**" />

  <Partition id="**sml**" size="**1**" />

  <Partition id="**sml\_bak**" size="**1**" />

  <Partition id="**uboot**" size="**1**" />

  <Partition id="**uboot\_bak**" size="**1**" />

  <Partition id="**logo**" size="**1**" />

  <Partition id="**fbootlogo**" size="**1**" />

  <Partition id="**l\_fixnv1**" size="**1**" />

  <Partition id="**l\_fixnv2**" size="**1**" />

  <Partition id="**l\_runtimenv1**" size="**1**" />

  <Partition id="**l\_runtimenv2**" size="**1**" />

  <Partition id="**gpsgl**" size="**1**" />

  <Partition id="**gpsbd**" size="**1**" />

  <Partition id="**wcnmodem**" size="**10**" />

  <Partition id="**persist**" size="**2**" />

  <Partition id="**l\_modem**" size="**25**" />

  <Partition id="**l\_gdsp**" size="**10**" />

  <Partition id="**l\_ldsp**" size="**20**" />

  <Partition id="**pm\_sys**" size="**1**" />

  <Partition id="**boot**" size="**20**" />

  <Partition id="**system**" size="**1080**" />

  <Partition id="**cache**" size="**150**" />

  <Partition id="**usbmsc**" size="**1100**" />

  <Partition id="**userdata**" size="**0xFFFFFFFF**" />

**Userdata** -- data partiton (Total size - all other partition size)

If you want to change size of system or usbmsc partition, modify below mk file:

/device/sprd/sharkle/sp9820e\_2c10/BoardConfig.mk

BOARD\_SYSTEMIMAGE\_PARTITION\_SIZE := 1073741824 // system

BOARD\_CACHEIMAGE\_PARTITION\_SIZE := 150000000 // cache

BOARD\_PRODNVIMAGE\_PARTITION\_SIZE := 5242880 // prodnv

BOARD\_USBMSCIMAGE\_PARTITION\_SIZE := 1073741824 #1G // usbmsc